#####################
  MA-7 Music Sample
#####################

<Cording Procedure>
1. Write a SMF file.
     MA7_Sample.mid

2. Import the SMF file into Authoring Tool.
     Import 'MA7_Sample.mid' file by selecting [File] - [Import SMF...].

3. Paste an Audio Data. (Data loading and its assignment.)
     As using 4-bit ADPCM Audio data in this example,
     set '16bit PCM Audio File Conversion' as '4bit ADPCM'
     by [Preference] in [Option] menu, in advance.
     Select Audio tab in Contents window,
     click-double the Audio ID #1 column to load '01_Loop.wav',
     click-double the Audio ID #2 column to load '02_Voice1.wav', and
     click-double the Audio ID #3 column to load '03_Voice2.wav'.

4. Play and check the sound generation is as expected.

5. Add Effect.
     Select Effect tab in Contents window,
     click-right over SFX1 ID #1 to select [Paste from Library/Effect List] - [KARAOKE2] - [KARAOKE2], and
     click-right over SFX2 ID #1 to select [Paste from Library/Effect List]
- [CHORUS1] - [CHORUS1].

6. Play and check the sound generation is as expected.
     Effect has been activated.

7. Add 3D Positioning.
     Click-right on 3D Track, 2nd measure, 1st beat, 0 tick (2:1:0), and
     select [Paste from Library/3D Pattern] - [No.41 : CounterClockwis2].
     When '3D ID Reassign' dialog appears, don't change anything and press 'OK'.
     (This case is assuming not to change 3D ID.)
     Similarly, select [No.41 : CounterClockwis2] at 5th measure, 1st beat,
     0 tick (5:1:0) and 8th measure, 1st beat, 0 tick (8:1:0).

     Put a checkmark to [3D Enable] on Contents window.
     Click [Edit 3D Patch] to open Patch Edit dialog.
     Set 'ID 0' on Audio #16 to assign 3D on Audio #16, the track '01_Loop.wav' is set.

8. Play and check the sound generation is as expected.
     You may sense that 3D is applied on the sound of Audio #16, '01_Loop.wav'.

9. Check the channel to synchronize with VS and/or LED, as necessary.
     Choose Tr. Status tab in Contents window and
click VS checkbox of Track Normal 5 to check them.
     Also, check R and B LED checkbox of Track Normal 3.
     (Set VS as #5 and LED as #3.)

10. Save as a project file (.m7p).
      Choose [Save] or [Save As...] from [File] menu.
      'MA7_Sample.m7p' may have been built.

11. Save as a SMAF file (.mmf).
      Choose [File] - [Export] - [Export SMAF...].
      'MA7_Sample.mmf' may have been corded.
